

**ArchiCAD - Adding TreCe gsm files to the Embedded Library**

1. File > Libraries and Objects > Library Manager…




1. Change the tab to “Embedded Library”
2. **Method I - Browse the folder**





* 1. Click “Add new folder”
  2. Browse to the folder “TreCe KLOSS - Embedded Library” on your hard disk and click “OK”
  3. Click “Reload & Apply” then “OK”

1. **Method II - Drag and drop**
   1. Browse (in the Windows Explorer) to the folder “TreCe KLOSS - Embedded Library” on your hard disk
   2. Drag and drop the folder “TreCe KLOSS - Embedded Library” into the Embedded Objects folder of the Library Manager
   3. Click “Reload & Apply” then “OK”




1. **Integrating associated materials**
   1. Open Options > Element Attributes > Attribute Manager > Surfaces





* 1. Click “Import”
  2. Browse for the “SURFACE.xml” then “Open” - Load attributes from the XML file
  3. Mark them all and add them to current project attributes “BY INDEX”
  4. OK -> Apply and Close



1. **Inserting objects**
   1. Double-click the “Object” tool



* 1. Browse to the “Embedded Library” and choose the object you want to add